Suggested Specification: IDM 6301

• Compliance with ICAO: Annex 14 Volume I 6th edition July 2013 paragraph 5.3.22.

• Elevated unidirectional flashing runway guard light for configuration A installations.