Suggested Specification: IDM 5848

* Compliance with ICAO: Annex 14 Volume I 6th edition July 2013
* Aerodrome Design Manual Part 4 Visual Aids, 4rd edition 2004
* FAA AC 150/5345-46D L-862
* High intensity bidirectional elevated light for:
	+ Runway Edge
	+ Threshold and end light (non-precision approach runways)