Suggested Specification: IDM 4562

* Compliance with:
	+ ICAO: Annex 14 Volume I 6th edition July 2013
	+ FAA AC 150 / 5345 - 46D
	+ Aerodrome Design Manual Part 4 Visual Aids, 4rd edition 2004
* High-intensity bidirectional inset light for:
	+ Bidirectional runway center line